Camera Setting  IP 
Camera For Dahua URL:  http://{0}/cgi-bin/snapshot.cgi?chn={1}&u={2}&p={3}  
 {0} - Static IP With Port  
 {1} - Channnel 
   {2} - UserName 
  {3} - Password
 IP Camera For Hikvision URL:  http://{0}/Streaming/Channels/{1}/picture    
{0} - Static IP With Port   
 {1} - Channnel 
 If You Check Static IP Work Or Not    
 https://www.yougetsignal.com/tools/open-ports/
 Check IP In URL If Its Work
 Get Rights Of Camera Setting 
Type:      Select Type (Dahua/Hikvision) 
HostName:  Static IP With Port (Example 122.230.410.812:8092)